**ECE 4723 Lab 3 Schematic Errata**

Andrew Bullington, Zach Fauver, Jesse Tutor, Will Gaines

The RTS# pin (pin 6) of the FTDI header requires a jumper to the MCLR pin (pin 1) of the ICSP header. This is required as the RTS# pin is not connected and is used for resetting the board on programming.

The RXD pin (pin 5) of the FTDI header requires a jumper to the RF0 pin located in the H1 header. This is required as the pin RXD is connected to by default is a input pin instead of an output pin.